**RFP** 23-5677

# Annex 5: FINANCIAL PROPOSAL SUBMISSION FORM

|  |
| --- |
| ***Portable drilling rig for atoll environments, Tuvalu***  |
| Goods description | Quantity required | Price USD | Total quantity | Total Amount USD |
| Man portable drill rig and components required for drilling of investigation holes and monitoring bores to a depth of 30m. | 1 drill rig and components for drilling investigation holes and monitoring bores | *[unit price]* | *[quantity]* | *[total amount]* |
| Drill rods, consideration for options hollow flight augers, and coring for 3m at base of holes  | Min 50m drill rods, costing for hollow flight augers and coring if an option | *[unit price]* | *[quantity]* | *[total amount]* |
| Tools/equipment required for operation of drill rig. Includes equipment needed for drilling, developing, and constructing monitoring bores, such as, but not restricted to additional compressor or pumps not provided with drill rig, but required for construction of monitoring bores.Excludes consumables such as casings, piezometer materials, gravels | One set of tools and equipment required for operation of drill rig and drilling of investigation holes, developing, and constructing monitoring bores as indicated. | *[unit price]* | *[quantity]* | *[total amount]* |
| Spare parts for 2 years operation of drill rig under normal operation. | Spare parts required in the first 2 years under normal operation | *[unit price]* | *[quantity]* | *[total amount]* |
| Consumables for 2 years operation of the drilling rig this would include filters, engine oil, gear oil, transmission and hydraulic fluids, replacement accessories, drilling muds and anything else deemed necessary by the bidder, under normal operation | Consumables required for first 2 years of operation under normal conditions | *[unit price]* | *[quantity]* | *[total amount]* |
| Training and testing of the drill rig onsite  | 10 days training and testing of drill rig. | *[unit price]* | *[quantity]* | *[total amount]* |
| Recommendations for the materials and installation of piezometers  | Materials and equipment for the installation of 34/28 mm (1”) as nested piezometers for up to 40 piezometers across 10 sites with up to 4 nested piezometers per site with depths up to 25m | *[unit price]* | *[quantity]* | *[total amount]* |
| Shipping and storage container | 1 container (20’) large enough to fit rig, spare parts and consumables | *[unit price]* | *[quantity]* | *[total amount]* |
|  | **Total Package 1** | *[Total 1]* |

|  |
| --- |
| **For the Bidder:** *[insert name of the company]* |
| Signature:Name of the representative: *[insert name of the representative]*Title: *[insert Title of the representative]* |
| Date: *[Click or tap to enter a date]* |